# Digital Sight 10 ver1.20 Update

## Changes
- Lessened horizontal artifacts which may appear under certain conditions.

## Update procedure
1. Connect the camera to PC via USB and turn on the camera.
2. Start "DsCamUpdater".
3. Click "UPDATE" button. Update process will start immediately.
   Important:
   Do not turn off the camera until update is completed.
   The update may fail, and the camera may not start normally.
4. When the update is completed,"The camera update is completed." will be displayed. Click OK.
5. Click Finish to close the DsCamUpdater. The update will take effect when restart the camera.


## About DsCamUpdater
DsCamUpdater incorporates third party material from the projects listed below.

- MaterialDesignInXamlToolkit
  Copyright (c) James Willock,  Mulholland Software and Contributors
  MIT License (https://opensource.org/licenses/mit-license.php)

- DynamicExpresso
  Copyright (c) 2018 Davide Icardi
  MIT License (https://opensource.org/licenses/mit-license.php)

- CalcBinding
  Apache License 2.0.(https://www.apache.org/licenses/LICENSE-2.0)

- - - 
Copyright (C) 2023 Nikon Corporation
